Location 906 "The default queuing is SP, and it is..." - according to this document - http://bizsupport1.austin.hp.com/bc/docs/support/SupportManual/c03187008/c03187008.pdf, page 46, the default queueing is WRR. 

Location 1506 + 1510 - the first reference says "clock summertime recurring", but then the config example says "clock summer-time CET repeating" - the use of "recurring" is for Cisco systems. "repeating" should be used for Comware.

Location 1853 - "line vty 04" - this should of course be "line vty 0 4"

Location 1893 - "username admin123 privilege 15 password verysecret" - this should use username secret, not username password (since we're talking about security).

Location 2032 "CDP is in read-only mode" - should say "CDP is in receive-only mode"

Location 2195 - answers A & D. I disagree with this - it should be C & D. SNMP templates are not used for actually setting communities on a device. 

Location 2367 - if a soft client is used, Voice Traffic can't be recognised by MAC OUI, as this will be the MAC of the PC. 

Location 3653/3658/3661 - first reference is to Bridge-aggregation 4, but then ports are assigned to group 3. Should be consistent.

Location 3702 - Answer A "..are HP A-Series and for a switch" - seems like sentence is cut off? 

Location 3733/3735/3738 - first reference is to Port-channel 10, but then interfaces are assigned to channel-group 1.

Location 3988 - "STP is fully compatible with RSTP bridges, in that an MSTP BPDU..." - I believe this should be "MSTP is fully compatible with RSTP bridges..."

Location 4371 - "Enable PortFast on all access ports:
Cisco (config)# ,
On Cisco switches to implement MSTP..."

The config command is missing here - should be "spanning-tree portfast default"

Location 4480 - the instance to VLAN mappings are different between HP & Cisco. Is that intentional? Unclear, since question is trying to get us to notice that STP is not enabled on the HP

Location 6467 - "Although VRRP support is not widely supported..." - Firstly should be "Although VRRP is not widely supported...", secondly it is now pretty widely supported. All routers should now support it, and have done since 12.2T days at least.

Location 7279 - "ospf authentication-mode md5 1...
cipher cant_find" - I don't think this should be broken across two lines

Location 7577 - "area-range 10.0.2.0 0.0.0.255 not-advertise"  - this should be something like "area 0 range 10.0.2.0 0.0.0.255 not-advertise" 

Location 8412 - "stub 10 no-summary" - I don't believe the "10" is required here.

Location 8572 - Answer E will work on a Cisco router. 

Location 8669 - "address 15.6.7.9 30" - should be "ip address 15.6.7.9 30"

Location 8708 - there should be an "ip nat outside" statement on the outside interface.

Location 9054 - "rule permit source 10.1.1.0 0.0.255.255" - I'm not sure, but this might be meant to only be "rule permit source 10.1.1.0 0.0.0.255" - i.e. matching the /24, not the /16

Location 13625 - "Which of the following is not the reason that HP-A..." - I don't think that "not" belongs here.

Locations 13660/14014 - the questions lists options A->G, but the answers only talk about A-D. I think that some of the answers should have multiple lines - e.g. the first two lines should be answer A.